Information provided to vendors during the walkthrough:

* The cable runs can all go back to the closest networking rack for each install.
* For the 32 cable runs to the computer lab at the High School, the existing runs will have to be removed in order for the installation to be completed properly.