Excelsior Springs Walkthrough Information

**Erate Project A - Fiber**

* All fiber should terminate inside a rack mounted LIU
* All fiber runs should be 6 strand OM3
* All fiber runs should originate in MDF
* All fiber connections should be LC
* Include 6 1M LC-LC OM3 patch cables
* HS Rooms 65 & 502 (see map)
* MS Room 407 (see map)

Questions:

* **Is there existing fiber at these locations?** Only 1 (HS Rm 502) where it is 1Gb fiber. The others are replacing copper.
* **Can we use an existing LIU in the HS MDF?** Yes.