Replace all existing racks/cabinets in existing IDF locations with new Hoffman Cabinet of appropriate size.

Please provide a separate quote for each building

Please provide a UPS for each cabinet.

Racks laid out patch panel then switch alternating configuration.

Integrator will be responsible for patching each rack.

Run 12 strand Fiber to each IDF location from the MDF.

Remove all existing copper cable and fiber.

Neosho High School  
IDF 5 will require 18 strands of fiber.

Goodman Elementary School  
IDF 2 will be a new IDF location.