**Q1: Are there any high density areas?**

A1: Yes. Common areas (ie, Gymnasiums, Theaters & Cafeterias) may have a larger number of clients connected than the standard classrooms.

**Q2: Are the current switches POE+**

A2: Yes.

**Q3. Should courtyards have WiFi as well?**

A3: No.

**Q4. How many APs are in the Gymnasiums?**

A4: CHS = 3, WMS = 1, GLN = 2, CPT = 1, MER, 1.

**Q5: Is a higher grade AP needed at the High School verse a standard classroom AP?**

A5: A higher grade AP is not required. However, the high school’s daily utilization is naturally higher than the other schools. If you recommend a higher grade AP due to this reality, please clearly define this as an option.

**Q6: Are protective cages required on APs in the Gymnasiums?**

A6: Yes. We recommend that you add a cage and mounting brackets in your bid for all Gymnasium APs.