FIBER DETAILS

Crawford ES: 2 - 6 strand Single Mode OS2 fiber lines x3 locations

London ES: 2 - 6 strand Single Mode OS2 fiber lines x2 locations

Oakland ES: 2 - 6 strand Single Mode OS2 fiber lines x5 locations

Sequoyah ES: 2 - 6 strand Single Mode OS2 fiber lines x2 locations

RMS: 2 - 6 strand Single Mode OS2 fiber lines x4 locations

RJHS:  2 - 6 strand Single Mode OS2 fiber lines x2 locations AND

             2 - 30+ strand Single Mode OS2 fiber lines x2 locations

             (2 lines minimum per location with 15+ strands per line.  More, smaller strand count lines acceptable as long as 60+ strands are given.  Ex: 10 - 6 strand lines per location)

Center Valley ES: 2 - 6 strand Single Mode OS2 fiber lines x1 location

Gardner: 2 - 6 strand Single Mode OS2 fiber lines x2 locations

RHS: 2 - 6 strand Single Mode OS2 fiber lines x7 locations

          2 - 24 strand Single Mode OS2 fiber lines x1 location

          inter-building: 2 - 6 strand Single Mode OS2 fiber lines x2 locations (Fine Arts, ATCC)

Fine Arts: 2 - 6 strand Single Mode OS2 fiber lines x3 locations

ATCC: 2 - 6 strand Single Mode OS2 fiber lines x4 locations