**PAC IDF:**

4 cameras (Erate ineligible)

2 WAPs

13 Standard Data Drops (Including spares for Access Control and potential BAS)

Total Anticipated Drops: 21

**New IDF 6-194 (COVERS BOTH FLOORS OF ADDITION)**

14 cameras (Erate ineligible)

13 WAPs

91 AV Data Drops (Erate ineligible)

22 Data Drops  (including spares for Access Control and Potential BAS)

Total Anticipated Drops: 134

**MDF**

12 Data Drops (these are solely for the IP PA/Bell/Clock system modules that will be added) (Erate ineligible)

Total Anticipated Drops: 12

**Fiber:**

2 new OS2 runs from MDF. 1 for existing PAC IDF and 1 for new IDF 6-194.

4 new powered fiber runs to pole mounted cameras.(Erate ineligible)