Tue 9-25-18 Yocum Walkthrough Questions and Answers

1. Where is the front Entrance to Yocum Elementary on the map?

The Front Entrance is newer than the map. The front Entrance isn’t on the map.

1. DO we run new surface mount conduit or use the old Aluminum.

Use existing conduits where you can.

1. Can we set surface box (on/or?) existing conduit.

As long as it is contact or the space in between has conduit.

1. Do we use Ivory or white boxes?

Use Ivory boxes.

1. Do we take down the old boxes where new wiring is going that is not in the Aluminum conduit?

Yes.

1. If the old cafeteria AP wiring is staying where do you want the new wiring?

Put cafeteria AP wiring on opposite wall.

1. In the principal's office at the Elementary does wiring go inside partition walls that can have boxes inside the the walls?

Yes..

1. Due to space restrictions in the conduit between floors do you want to use Fiber?

Yes..

1. Where do you want to terminate fiber?

All fiber back to MDF.

1. What type of fiber between building, single or multi-mode?

Single mode.

1. Do you have an objection to trenching?

Trenched outside fences bored inside. Bored under road.

1. To make the run less expensive to the district and the path the fiber follows between buildings be altered?

Yes.

1. What is the part number for the cable run patches for the Primary lab and IDF?

Part #Leviton 41D6A-1F4

Thursday 10-4-2018 Yocum Walkthrough Questions and Answers

1. Are the vendors supplying patch cables?

 Yes CAT6A of sufficient Length to reach from patch panel to switch and sufficient quantity have enough for every port in matching color to the port.

2. Is there a problem with conduit on the outside of the building to get the fiber from burial to the MDF?

 No, there is already conduit and other non original features applied to the outside of the building on that side, although we do expect a reasonable effort to keep appearances unobtrusive and unobtrusive.

3.Are there any other Fiber runs being replaced besides the one between Yocum Elementary and Yocum Primary?

No other fiber is required to be replaced,but, the Vendor may choose to run fiber between floor and or to any IDF.